#!/usr/local/bin/bdmctrl -D2
#
# firebee board initialization for bdmctrl 
#
open $1
reset
sleep 1

wait

# use system sdram as flashlib scratch area.
# TODO: plugin flashing seems to work o.k. now for smaller binaries, while it doesn't for larger ones (EmuTOS) yet.
# This seems to be related to large flash buffers and PC-relative adressing of the plugin
#flash-plugin 0x1000 0xf000 flash29-5475.plugin
# notify flashlib that we have flash at address 0xE0000000, length 0x7FFFFF, plugin is flash29
flash 0xe0000000

# Erase flash from 0xE0000000 to 0xE00FFFFF (reserved space for BaS)
#
# Caution: sector offset numbers need to be the ones from the x16 address range
# column and they vary in size - needs to be exactly as in the data sheet (p. 9)
#

erase 0xe0000000 0
erase 0xe0000000 0x1000
erase 0xe0000000 0x2000
erase 0xe0000000 0x3000
erase 0xe0000000 0x4000
erase 0xe0000000 0x5000
erase 0xe0000000 0x6000
erase 0xe0000000 0x7000
erase 0xe0000000 0x8000
erase 0xe0000000 0x10000
erase 0xe0000000 0x18000
erase 0xe0000000 0x20000
erase 0xe0000000 0x28000
erase 0xe0000000 0x30000
erase 0xe0000000 0x38000
erase 0xe0000000 0x40000
erase 0xe0000000 0x48000
erase 0xe0000000 0x50000
erase 0xe0000000 0x58000
erase 0xe0000000 0x60000
erase 0xe0000000 0x70000
erase 0xe0000000 0x78000

erase-wait 0xe0000000
# should now have erased from 0xe0000000 to 0xe00fffff

dump-mem 0xe0010000 0x20 b

load -v ../firebee/bas.elf
wait
