Begin4
Title:		bdm-load
Version:	030815
Entered-date:	2003-08-15
Description:	Flash writer utility for 683xx target systems through
		Background Debug Mode interface for Motorola CPU32 and Linux
		Both Public Domain and ICD interfaces are supported.
		Code contains first experimental tests of GPLed TPU debugger
		project.
		* More info about related software and BDM driver at
		    http://cmp.felk.cvut.cz/~pisa
		    http://cmp.felk.cvut.cz/~pisa/m683xx/bdm_driver.html
Keywords:	debugger GDB m68k 68332 683xx BDM flash embedded TPU
Author:		jeff@uclinux.org (D.Jeff Dionne)
		adennison@swin.edu.au (Andrew Dennison)
		pisa@cvlinux.felk.cvut.cz (Pavel Pisa)
Maintained-by:	pisa@cvlinux.felk.cvut.cz (Pavel Pisa)
Primary-site:	metalab.unc.edu /pub/Linux/devel/debuggers
		210 kB bdm-load-030519.tar.gz
Alternate-site:	ftp.cygnus.com /pub/embedded
		210 kB bdm-load-030519.tar.gz
Original-site:	freeware.aus.sps.mot.com
Platforms:	Linux 2.0.xx, 2.2.yy, 2.4.zz ( last tested 2.5.69 )
Copying-policy:	GPL
End
