/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/
/*
Copyright (C) 1991-2010 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.
*/
(header "symbol" (version "1.1"))
(symbol
	(rect 0 0 376 232)
	(text "altpll4" (rect 168 1 215 20)(font "Arial" (font_size 10)))
	(text "inst" (rect 8 213 31 228)(font "Arial" ))
	(port
		(pt 0 72)
		(input)
		(text "inclk0" (rect 0 0 40 16)(font "Arial" (font_size 8)))
		(text "inclk0" (rect 4 56 38 72)(font "Arial" (font_size 8)))
		(line (pt 0 72)(pt 88 72)(line_width 1))
	)
	(port
		(pt 0 96)
		(input)
		(text "areset" (rect 0 0 42 16)(font "Arial" (font_size 8)))
		(text "areset" (rect 4 80 40 96)(font "Arial" (font_size 8)))
		(line (pt 0 96)(pt 88 96)(line_width 1))
	)
	(port
		(pt 0 120)
		(input)
		(text "scanclk" (rect 0 0 53 16)(font "Arial" (font_size 8)))
		(text "scanclk" (rect 4 104 49 120)(font "Arial" (font_size 8)))
		(line (pt 0 120)(pt 88 120)(line_width 1))
	)
	(port
		(pt 0 144)
		(input)
		(text "scandata" (rect 0 0 62 16)(font "Arial" (font_size 8)))
		(text "scandata" (rect 4 128 57 144)(font "Arial" (font_size 8)))
		(line (pt 0 144)(pt 88 144)(line_width 1))
	)
	(port
		(pt 0 168)
		(input)
		(text "scanclkena" (rect 0 0 77 16)(font "Arial" (font_size 8)))
		(text "scanclkena" (rect 4 152 70 168)(font "Arial" (font_size 8)))
		(line (pt 0 168)(pt 88 168)(line_width 1))
	)
	(port
		(pt 0 192)
		(input)
		(text "configupdate" (rect 0 0 86 16)(font "Arial" (font_size 8)))
		(text "configupdate" (rect 4 176 77 192)(font "Arial" (font_size 8)))
		(line (pt 0 192)(pt 88 192)(line_width 1))
	)
	(port
		(pt 376 72)
		(output)
		(text "c0" (rect 0 0 16 16)(font "Arial" (font_size 8)))
		(text "c0" (rect 359 56 373 72)(font "Arial" (font_size 8)))
		(line (pt 376 72)(pt 288 72)(line_width 1))
	)
	(port
		(pt 376 96)
		(output)
		(text "scandataout" (rect 0 0 83 16)(font "Arial" (font_size 8)))
		(text "scandataout" (rect 302 80 373 96)(font "Arial" (font_size 8)))
		(line (pt 376 96)(pt 288 96)(line_width 1))
	)
	(port
		(pt 376 120)
		(output)
		(text "scandone" (rect 0 0 66 16)(font "Arial" (font_size 8)))
		(text "scandone" (rect 317 104 373 120)(font "Arial" (font_size 8)))
		(line (pt 376 120)(pt 288 120)(line_width 1))
	)
	(port
		(pt 376 144)
		(output)
		(text "locked" (rect 0 0 44 16)(font "Arial" (font_size 8)))
		(text "locked" (rect 335 128 373 144)(font "Arial" (font_size 8)))
		(line (pt 376 144)(pt 288 144)(line_width 1))
	)
	(drawing
		(text "Cyclone III" (rect 301 214 349 228)(font "Arial" ))
		(text "inclk0 frequency: 48.000 MHz" (rect 98 123 241 137)(font "Arial" ))
		(text "Operation Mode: Normal" (rect 98 140 213 154)(font "Arial" ))
		(text "Clk " (rect 99 167 116 181)(font "Arial" ))
		(text "Ratio" (rect 125 167 149 181)(font "Arial" ))
		(text "Ph (dg)" (rect 159 167 194 181)(font "Arial" ))
		(text "DC (%)" (rect 204 167 239 181)(font "Arial" ))
		(text "c0" (rect 103 185 115 199)(font "Arial" ))
		(text "2/1" (rect 131 185 146 199)(font "Arial" ))
		(text "0.00" (rect 167 185 188 199)(font "Arial" ))
		(text "50.00" (rect 209 185 236 199)(font "Arial" ))
		(line (pt 0 0)(pt 377 0)(line_width 1))
		(line (pt 377 0)(pt 377 233)(line_width 1))
		(line (pt 0 233)(pt 377 233)(line_width 1))
		(line (pt 0 0)(pt 0 233)(line_width 1))
		(line (pt 96 164)(pt 246 164)(line_width 1))
		(line (pt 96 181)(pt 246 181)(line_width 1))
		(line (pt 96 199)(pt 246 199)(line_width 1))
		(line (pt 96 164)(pt 96 199)(line_width 1))
		(line (pt 122 164)(pt 122 199)(line_width 3))
		(line (pt 156 164)(pt 156 199)(line_width 3))
		(line (pt 201 164)(pt 201 199)(line_width 3))
		(line (pt 245 164)(pt 245 199)(line_width 1))
		(line (pt 88 56)(pt 288 56)(line_width 1))
		(line (pt 288 56)(pt 288 216)(line_width 1))
		(line (pt 88 216)(pt 288 216)(line_width 1))
		(line (pt 88 56)(pt 88 216)(line_width 1))
	)
)
