/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/
/*
Copyright (C) 1991-2008 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.
*/
(header "symbol" (version "1.1"))
(symbol
	(rect 0 0 152 192)
	(text "lpm_mux6" (rect 50 2 120 18)(font "Arial" (font_size 10)))
	(text "inst" (rect 8 176 25 188)(font "Arial" ))
	(port
		(pt 0 40)
		(input)
		(text "data7x[23..0]" (rect 0 0 74 14)(font "Arial" (font_size 8)))
		(text "data7x[23..0]" (rect 4 27 66 40)(font "Arial" (font_size 8)))
		(line (pt 0 40)(pt 72 40)(line_width 3))
	)
	(port
		(pt 0 56)
		(input)
		(text "data6x[23..0]" (rect 0 0 74 14)(font "Arial" (font_size 8)))
		(text "data6x[23..0]" (rect 4 43 66 56)(font "Arial" (font_size 8)))
		(line (pt 0 56)(pt 72 56)(line_width 3))
	)
	(port
		(pt 0 72)
		(input)
		(text "data5x[23..0]" (rect 0 0 74 14)(font "Arial" (font_size 8)))
		(text "data5x[23..0]" (rect 4 59 66 72)(font "Arial" (font_size 8)))
		(line (pt 0 72)(pt 72 72)(line_width 3))
	)
	(port
		(pt 0 88)
		(input)
		(text "data4x[23..0]" (rect 0 0 74 14)(font "Arial" (font_size 8)))
		(text "data4x[23..0]" (rect 4 75 66 88)(font "Arial" (font_size 8)))
		(line (pt 0 88)(pt 72 88)(line_width 3))
	)
	(port
		(pt 0 104)
		(input)
		(text "data3x[23..0]" (rect 0 0 74 14)(font "Arial" (font_size 8)))
		(text "data3x[23..0]" (rect 4 91 66 104)(font "Arial" (font_size 8)))
		(line (pt 0 104)(pt 72 104)(line_width 3))
	)
	(port
		(pt 0 120)
		(input)
		(text "data2x[23..0]" (rect 0 0 74 14)(font "Arial" (font_size 8)))
		(text "data2x[23..0]" (rect 4 107 66 120)(font "Arial" (font_size 8)))
		(line (pt 0 120)(pt 72 120)(line_width 3))
	)
	(port
		(pt 0 136)
		(input)
		(text "data1x[23..0]" (rect 0 0 74 14)(font "Arial" (font_size 8)))
		(text "data1x[23..0]" (rect 4 123 66 136)(font "Arial" (font_size 8)))
		(line (pt 0 136)(pt 72 136)(line_width 3))
	)
	(port
		(pt 0 152)
		(input)
		(text "data0x[23..0]" (rect 0 0 74 14)(font "Arial" (font_size 8)))
		(text "data0x[23..0]" (rect 4 139 66 152)(font "Arial" (font_size 8)))
		(line (pt 0 152)(pt 72 152)(line_width 3))
	)
	(port
		(pt 0 168)
		(input)
		(text "clock" (rect 0 0 29 14)(font "Arial" (font_size 8)))
		(text "clock" (rect 4 155 27 168)(font "Arial" (font_size 8)))
		(line (pt 0 168)(pt 72 168)(line_width 1))
	)
	(port
		(pt 80 192)
		(input)
		(text "sel[2..0]" (rect 0 0 44 14)(font "Arial" (font_size 8)))
		(text "sel[2..0]" (rect 84 179 121 192)(font "Arial" (font_size 8)))
		(line (pt 80 192)(pt 80 180)(line_width 3))
	)
	(port
		(pt 152 104)
		(output)
		(text "result[23..0]" (rect 0 0 67 14)(font "Arial" (font_size 8)))
		(text "result[23..0]" (rect 92 91 147 104)(font "Arial" (font_size 8)))
		(line (pt 152 104)(pt 88 104)(line_width 3))
	)
	(drawing
		(line (pt 72 24)(pt 72 184)(line_width 1))
		(line (pt 88 32)(pt 88 176)(line_width 1))
		(line (pt 72 24)(pt 88 32)(line_width 1))
		(line (pt 72 184)(pt 88 176)(line_width 1))
		(line (pt 72 162)(pt 78 168)(line_width 1))
		(line (pt 78 168)(pt 72 174)(line_width 1))
	)
)
