/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/
/*
Copyright (C) 1991-2008 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.
*/
(header "symbol" (version "1.1"))
(symbol
	(rect 0 0 240 136)
	(text "altddio_bidir0" (rect 82 1 171 17)(font "Arial" (font_size 10)))
	(text "inst" (rect 8 120 25 132)(font "Arial" ))
	(port
		(pt 0 24)
		(input)
		(text "datain_h[31..0]" (rect 0 0 83 14)(font "Arial" (font_size 8)))
		(text "datain_h[31..0]" (rect 4 11 76 24)(font "Arial" (font_size 8)))
		(line (pt 0 24)(pt 88 24)(line_width 3))
	)
	(port
		(pt 0 40)
		(input)
		(text "datain_l[31..0]" (rect 0 0 79 14)(font "Arial" (font_size 8)))
		(text "datain_l[31..0]" (rect 4 27 73 40)(font "Arial" (font_size 8)))
		(line (pt 0 40)(pt 88 40)(line_width 3))
	)
	(port
		(pt 0 56)
		(input)
		(text "oe" (rect 0 0 14 14)(font "Arial" (font_size 8)))
		(text "oe" (rect 4 43 16 56)(font "Arial" (font_size 8)))
		(line (pt 0 56)(pt 88 56)(line_width 1))
	)
	(port
		(pt 0 72)
		(input)
		(text "inclock" (rect 0 0 38 14)(font "Arial" (font_size 8)))
		(text "inclock" (rect 4 59 36 72)(font "Arial" (font_size 8)))
		(line (pt 0 72)(pt 88 72)(line_width 1))
	)
	(port
		(pt 0 88)
		(input)
		(text "outclock" (rect 0 0 47 14)(font "Arial" (font_size 8)))
		(text "outclock" (rect 4 75 42 88)(font "Arial" (font_size 8)))
		(line (pt 0 88)(pt 88 88)(line_width 1))
	)
	(port
		(pt 240 24)
		(output)
		(text "dataout_h[31..0]" (rect 0 0 92 14)(font "Arial" (font_size 8)))
		(text "dataout_h[31..0]" (rect 159 11 237 24)(font "Arial" (font_size 8)))
		(line (pt 240 24)(pt 144 24)(line_width 3))
	)
	(port
		(pt 240 40)
		(output)
		(text "dataout_l[31..0]" (rect 0 0 87 14)(font "Arial" (font_size 8)))
		(text "dataout_l[31..0]" (rect 163 27 238 40)(font "Arial" (font_size 8)))
		(line (pt 240 40)(pt 144 40)(line_width 3))
	)
	(port
		(pt 240 72)
		(output)
		(text "combout[31..0]" (rect 0 0 83 14)(font "Arial" (font_size 8)))
		(text "combout[31..0]" (rect 166 59 237 72)(font "Arial" (font_size 8)))
		(line (pt 240 72)(pt 144 72)(line_width 3))
	)
	(port
		(pt 240 56)
		(bidir)
		(text "padio[31..0]" (rect 0 0 66 14)(font "Arial" (font_size 8)))
		(text "padio[31..0]" (rect 181 43 238 56)(font "Arial" (font_size 8)))
		(line (pt 240 56)(pt 144 56)(line_width 3))
	)
	(drawing
		(text "ddio" (rect 108 27 129 40)(font "Arial" (font_size 8)))
		(text "bidir" (rect 108 42 129 55)(font "Arial" (font_size 8)))
		(text "power up" (rect 92 90 129 102)(font "Arial" ))
		(text "low" (rect 92 100 105 112)(font "Arial" ))
		(line (pt 88 16)(pt 144 16)(line_width 1))
		(line (pt 144 16)(pt 144 112)(line_width 1))
		(line (pt 144 112)(pt 88 112)(line_width 1))
		(line (pt 88 112)(pt 88 16)(line_width 1))
	)
)
