-- megafunction wizard: %LPM_SHIFTREG%
-- GENERATION: STANDARD
-- VERSION: WM1.0
-- MODULE: lpm_shiftreg 

-- ============================================================
-- File Name: lpm_shiftreg0.tdf
-- Megafunction Name(s):
-- 			lpm_shiftreg
--
-- Simulation Library Files(s):
-- 			lpm
-- ============================================================
-- ************************************************************
-- THIS IS A WIZARD-GENERATED FILE. DO NOT EDIT THIS FILE!
--
-- 9.1 Build 350 03/24/2010 SP 2 SJ Web Edition
-- ************************************************************


--Copyright (C) 1991-2010 Altera Corporation
--Your use of Altera Corporation's design tools, logic functions 
--and other software and tools, and its AMPP partner logic 
--functions, and any output files from any of the foregoing 
--(including device programming or simulation files), and any 
--associated documentation or information are expressly subject 
--to the terms and conditions of the Altera Program License 
--Subscription Agreement, Altera MegaCore Function License 
--Agreement, or other applicable license agreement, including, 
--without limitation, that your use is for the sole purpose of 
--programming logic devices manufactured by Altera and sold by 
--Altera or its authorized distributors.  Please refer to the 
--applicable agreement for further details.

INCLUDE "lpm_shiftreg.inc";



SUBDESIGN lpm_shiftreg0
(
	clock	 : INPUT;
	shiftin	 : INPUT;
	shiftout	 : OUTPUT;
)

VARIABLE

	lpm_shiftreg_component : lpm_shiftreg WITH (
			LPM_DIRECTION = "LEFT",
			LPM_TYPE = "LPM_SHIFTREG",
			LPM_WIDTH = 16
			);

BEGIN

	shiftout = lpm_shiftreg_component.shiftout;
	lpm_shiftreg_component.clock = clock;
	lpm_shiftreg_component.shiftin = shiftin;
END;



-- ============================================================
-- CNX file retrieval info
-- ============================================================
-- Retrieval info: PRIVATE: ACLR NUMERIC "0"
-- Retrieval info: PRIVATE: ALOAD NUMERIC "0"
-- Retrieval info: PRIVATE: ASET NUMERIC "0"
-- Retrieval info: PRIVATE: ASET_ALL1 NUMERIC "1"
-- Retrieval info: PRIVATE: CLK_EN NUMERIC "0"
-- Retrieval info: PRIVATE: INTENDED_DEVICE_FAMILY STRING "Cyclone III"
-- Retrieval info: PRIVATE: LeftShift NUMERIC "1"
-- Retrieval info: PRIVATE: ParallelDataInput NUMERIC "0"
-- Retrieval info: PRIVATE: Q_OUT NUMERIC "0"
-- Retrieval info: PRIVATE: SCLR NUMERIC "0"
-- Retrieval info: PRIVATE: SLOAD NUMERIC "0"
-- Retrieval info: PRIVATE: SSET NUMERIC "0"
-- Retrieval info: PRIVATE: SSET_ALL1 NUMERIC "1"
-- Retrieval info: PRIVATE: SYNTH_WRAPPER_GEN_POSTFIX STRING "0"
-- Retrieval info: PRIVATE: SerialShiftInput NUMERIC "1"
-- Retrieval info: PRIVATE: SerialShiftOutput NUMERIC "1"
-- Retrieval info: PRIVATE: nBit NUMERIC "16"
-- Retrieval info: CONSTANT: LPM_DIRECTION STRING "LEFT"
-- Retrieval info: CONSTANT: LPM_TYPE STRING "LPM_SHIFTREG"
-- Retrieval info: CONSTANT: LPM_WIDTH NUMERIC "16"
-- Retrieval info: USED_PORT: clock 0 0 0 0 INPUT NODEFVAL clock
-- Retrieval info: USED_PORT: shiftin 0 0 0 0 INPUT NODEFVAL shiftin
-- Retrieval info: USED_PORT: shiftout 0 0 0 0 OUTPUT NODEFVAL shiftout
-- Retrieval info: CONNECT: @clock 0 0 0 0 clock 0 0 0 0
-- Retrieval info: CONNECT: @shiftin 0 0 0 0 shiftin 0 0 0 0
-- Retrieval info: CONNECT: shiftout 0 0 0 0 @shiftout 0 0 0 0
-- Retrieval info: LIBRARY: lpm lpm.lpm_components.all
-- Retrieval info: GEN_FILE: TYPE_NORMAL lpm_shiftreg0.tdf TRUE
-- Retrieval info: GEN_FILE: TYPE_NORMAL lpm_shiftreg0.inc TRUE
-- Retrieval info: GEN_FILE: TYPE_NORMAL lpm_shiftreg0.cmp TRUE
-- Retrieval info: GEN_FILE: TYPE_NORMAL lpm_shiftreg0.bsf TRUE FALSE
-- Retrieval info: GEN_FILE: TYPE_NORMAL lpm_shiftreg0_inst.tdf FALSE
-- Retrieval info: LIB_FILE: lpm
