/*
WARNING: Do NOT edit the input and output ports in this file in a text
editor if you plan to continue editing the block that represents it in
the Block Editor! File corruption is VERY likely to occur.
*/
/*
Copyright (C) 1991-2014 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.
*/
(header "symbol" (version "1.2"))
(symbol
	(rect 0 0 272 176)
	(text "altpll1" (rect 119 0 160 16)(font "Arial" (font_size 10)))
	(text "inst" (rect 8 161 26 172)(font "Arial" ))
	(port
		(pt 0 64)
		(input)
		(text "inclk0" (rect 0 0 34 13)(font "Arial" (font_size 8)))
		(text "inclk0" (rect 4 51 31 63)(font "Arial" (font_size 8)))
		(line (pt 0 64)(pt 40 64))
	)
	(port
		(pt 272 64)
		(output)
		(text "c0" (rect 0 0 15 13)(font "Arial" (font_size 8)))
		(text "c0" (rect 257 51 269 63)(font "Arial" (font_size 8)))
	)
	(port
		(pt 272 80)
		(output)
		(text "c1" (rect 0 0 14 13)(font "Arial" (font_size 8)))
		(text "c1" (rect 257 67 267 79)(font "Arial" (font_size 8)))
	)
	(port
		(pt 272 96)
		(output)
		(text "c2" (rect 0 0 15 13)(font "Arial" (font_size 8)))
		(text "c2" (rect 257 83 269 95)(font "Arial" (font_size 8)))
	)
	(port
		(pt 272 112)
		(output)
		(text "locked" (rect 0 0 37 13)(font "Arial" (font_size 8)))
		(text "locked" (rect 237 99 268 111)(font "Arial" (font_size 8)))
	)
	(drawing
		(text "Cyclone III" (rect 214 162 474 334)(font "Arial" ))
		(text "inclk0 frequency: 33.000 MHz" (rect 50 60 226 130)(font "Arial" ))
		(text "Operation Mode: Src Sync Comp" (rect 50 72 239 154)(font "Arial" ))
		(text "Clk " (rect 51 91 117 192)(font "Arial" ))
		(text "Ratio" (rect 71 91 165 192)(font "Arial" ))
		(text "Ph (dg)" (rect 98 91 227 192)(font "Arial" ))
		(text "DC (%)" (rect 133 91 298 192)(font "Arial" ))
		(text "c0" (rect 54 104 119 218)(font "Arial" ))
		(text "16/11" (rect 71 104 164 218)(font "Arial" ))
		(text "0.00" (rect 104 104 227 218)(font "Arial" ))
		(text "50.00" (rect 137 104 298 218)(font "Arial" ))
		(text "c1" (rect 54 117 118 244)(font "Arial" ))
		(text "16/33" (rect 71 117 165 244)(font "Arial" ))
		(text "0.00" (rect 104 117 227 244)(font "Arial" ))
		(text "50.00" (rect 137 117 298 244)(font "Arial" ))
		(text "c2" (rect 54 130 119 270)(font "Arial" ))
		(text "32/43" (rect 71 130 166 270)(font "Arial" ))
		(text "0.00" (rect 104 130 227 270)(font "Arial" ))
		(text "50.00" (rect 137 130 298 270)(font "Arial" ))
		(line (pt 0 0)(pt 273 0))
		(line (pt 273 0)(pt 273 177))
		(line (pt 0 177)(pt 273 177))
		(line (pt 0 0)(pt 0 177))
		(line (pt 48 89)(pt 165 89))
		(line (pt 48 101)(pt 165 101))
		(line (pt 48 114)(pt 165 114))
		(line (pt 48 127)(pt 165 127))
		(line (pt 48 140)(pt 165 140))
		(line (pt 48 89)(pt 48 140))
		(line (pt 68 89)(pt 68 140)(line_width 3))
		(line (pt 95 89)(pt 95 140)(line_width 3))
		(line (pt 130 89)(pt 130 140)(line_width 3))
		(line (pt 164 89)(pt 164 140))
		(line (pt 40 48)(pt 223 48))
		(line (pt 223 48)(pt 223 159))
		(line (pt 40 159)(pt 223 159))
		(line (pt 40 48)(pt 40 159))
		(line (pt 271 64)(pt 223 64))
		(line (pt 271 80)(pt 223 80))
		(line (pt 271 96)(pt 223 96))
		(line (pt 271 112)(pt 223 112))
	)
)
